Upper Yangtze River Scientific Data Center

**25km Soil Moisture Data Set in Southwest China Based on Microwave Data Assimilation (2002-2011)**

1、Description

The Chinese soil moisture data set based on microwave data assimilation includes three layers of soil moisture data (0-5cm, 5-20cm, 20-100cm) from 2002 to 2011. The land surface assimilation system (ITPLDAS) developed by Yang et al. Root mean square error of soil moisture: 5% VWC (assessment accuracy in Naqu and Maqu of Qinghai Tibet Plateau).

2、Keywords

Theme：Soil,Soil moisture,Terrestrial Surface Remote Sensing
Discipline：Terrestrial Surface
Places：Southwest China, China
Time：2002-2011

3、Data details

1.Scale：None

2.Projection：

3.Filesize：1800.0MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：35.0 | - |
| west：96.0 | - | east：113.0 |
| - | south：20.5 | - |

5、Time frame:None--None

6、Reference method

References to data:

YANG Kun. 25km Soil Moisture Data Set in Southwest China Based on Microwave Data Assimilation (2002-2011). Upper Yangtze River Scientific Data Center, 2022

References to articles:

阳坤. (2018). 基于微波数据同化的中国土壤水分数据集（2002-2011）. 国家青藏高原科学数据中心, DOI: 10.11888/AtmosphericPhysics.tpe.249448.file. CSTR: 18406.11.AtmosphericPhysics.tpe.249448.file

Yang, K., Chen, Y.Y., He, J., Zhao, L., Lu, H., Qin, J., Zheng, D.H., Li, X. (2020). Development of a daily soil moisture product for the period of 2002–2011 in Chinese Mainland. Science China - Earth Sciences, doi: 10.1007/s11430-019-9588-5

Yang, Kun, Zhu, La, Chen, Yingying, Zhao, Long, Qin, Jun, Lu, Hui, Tang, Wenjun, Han, Menglei, Ding, Baohong, Fang, Nan. Land surface model calibration through microwave data assimilation for improving soil moisture simulations. Journal of Hydrology, 2016, 533:266-276. doi:10.1016/j.jhydrol.2015.12.018

Yang, K., T. Koike, I. Kaihotsu, and J. Qin, 2009: Validation of a Dual-Pass Microwave Land Data Assimilation System for Estimating Surface Soil Moisture in Semiarid Regions, J. Hydrometeorol., 10(3), 780-793, doi:10.1175/2008JHM1065

Yang, K., Watanabe, T., Koike, T., Li, X., Fujii, H., Tamagawa, K., Ma, Y.M., &Ishikawa, H. (2007). Auto-calibration system developed to assimilate AMSR-E data into a land surface model for estimating soil moisture and the surface energy budget. Journal of The Meteorological Society of Japan, 85A, 229-242

7、Supporting project information

8、Data resource provider

name: YANG Kun
unit: Institute of Tibetan Plateau Research, Chinese Academy of Sciences
email: yangk@itpcas.ac.cn